}}BIT CLOCK RATE,WORD CLOCKGENERATORSCHEMATIC 113 BIT BINARYCOUNTERADDRESS EPROM WITH DATA FRAMEPROGRAM

SCHEMATIC 2SYNC WORD GENERATORSCHEMATIC 6POWERCONDITIONERSCHEMATIC 10CONTROLMODULE BLOCKDIAGRAM

WCLKBCLKDEVICE ENABLESERIAL OUTEND OF FRAMEWCLKBCLK8 BITDEVICEADDRESS+5V+12V+15VSERIAL DATA INSERIAL DATA OUT

BUS I/O BUFFERSSCHEMATIC 7

+15V and -15V POWERIN

PG 2PG 1PG 3

BUSSERIAL DATA OUTBI PHASETTLFRAME # 32 BITCOUNTERSCHEMATIC 4A, BINTERNAL DEVICESENABLE LINES8

8INTERNALDEVICEADDRESSDECODERSCHEMATIC 3INTERNALDEVICESSERIAL DATAEND OF FRAME

SERIAL TO BI PHASE DATA CONVERTERSCHEMATIC 5ISOP.S.SCHEMATIC 9OPTOCOUPLERSSCHEMATIC 8

UCB DATA ACQUISITION SYSTEMDAS